Rule:

--
Sid:
1814

--
Summary:
This event is generated when an attempt is made to exploit a flaw on a Cisco VoIP telephone.

--
Impact:
Denial of Service.

--
Detailed Information:
Certain versions of Cisco's VoIP phones are vulnerable to an attack that can cause them to reboot when they recieve an http request such as  http://ciscophoneip/StreamingStatistics?<value> where <value> is an  integer value of arbitrary high value, typically a number greater than  32768.

--
Affected Systems:
Cisco VoIP Phones 7910, 7940, and 7960 (software version 3.0 to 3.2)

--
Attack Scenarios:
A remote user can send the exploit url to the phone, causing the phone to reboot and disallowingthe user to place or recieve calls for up to 30 seconds.

--
Ease of Attack:
Simple.

--
False Positives: 
None known.

--
False Negatives: 
None known.

--
Corrective Action:
Apply the appropriate vendor supplied patches.

--
Contributors:
Sourcefire Vulnerability Research Team
Brian Caswell <bmc@sourcefire.com>
Nigel Houghton <nigel.houghton@sourcefire.com> 
Snort documentation contributed by Josh Sakofsky

-- 
Additional References:

--
